LiftMaster Distributed by ZeroDocs.com

**SECTION 28 10 00 – ACCESS CONTROL**

GENERAL

ADMINISTRATIVE REQUIREMENTS

Pre-Installation Conference:

Attendance: [Architect,] [Owner,] [Contractor,] [Construction Manager,] installer, and related trades.

Review: Project conditions, manufacturer requirements, delivery and storage, staging and sequencing, and protection of completed work.

SUBMITTALS

Action Submittals:

Shop Drawings: Illustrate products, installation, and relationship to adjacent construction.

Product Data: Manufacturer’s descriptive data and product attributes for metal panels and underlayment.

Samples: [Selection samples.] [Verification samples.]

Informational Submittals:

Certificate of Compliance: Certification that installed products meet specified design and performance requirements.

Closeout Submittals:

Operation and Maintenance Data.

QUALITY ASSURANCE

[Fabricator] [Installer] Qualifications: Minimum [2] [\_\_] years’ experience in work of this Section.

WARRANTY

Manufacturer’s 2 year warranty for telephone entry/access and perimeter control system.

PRODUCTS

MANUFACTURERS

Contract Documents are based on products by LiftMaster. [www.liftmaster.com](http://www.liftmaster.com/)

Substitutions: [Refer to Division 01.] [Not permitted.]

TELEPHONE ENTRY CONTROL SYSTEM

Commercial and Multi-Dwelling Unit Cloud Based Access Control/Telephone Entry System:

Model: CAPXS Smart Video Intercom - S

Local user capacity: 3,000.

Touch screen operation with USB integrated video camera.

* + - 1. One primary relay and auxiliary relays

Compatible with MyQ Community.

Internet connection: [High-speed CAT 5/6 IEEE 802.] [Wi-Fi IEEE 802.]

Accessories:

* + - * 1. CAP2D smart access two door controller.
        2. Trim plate for retrofit mounting.
        3. Trim plate with a postal lock provision for retrofit mounting.
        4. Sun protective hood.
        5. User application: myQ Community.

EXECUTION

INSTALLATION

Install in accordance with manufacturer’s instructions and approved Shop Drawings.

CLOSEOUT ACTIVITIES

Demonstration: Demonstrate system operation to Owner.

MAINTENANCE

Maintenance Service: Furnish service and maintenance of access control systems for period of 3 months after date of Substantial Completion.

END OF SECTION