LiftMaster Distributed by ZeroDocs.com

**SECTION 28 10 00 – ACCESS CONTROL**

GENERAL

ADMINISTRATIVE REQUIREMENTS

Pre-Installation Conference:

Attendance: [Architect,] [Owner,] [Contractor,] [Construction Manager,] installer, and related trades.

Review: Project conditions, manufacturer requirements, delivery and storage, staging and sequencing, and protection of completed work.

SUBMITTALS

Action Submittals:

Shop Drawings: Illustrate products, installation, and relationship to adjacent construction.

Product Data: Manufacturer’s descriptive data and product attributes for metal panels and underlayment.

Samples: [Selection samples.] [Verification samples.]

Informational Submittals:

Certificate of Compliance: Certification that installed products meet specified design and performance requirements.

Closeout Submittals:

Operation and Maintenance Data.

QUALITY ASSURANCE

[Fabricator] [Installer] Qualifications: Minimum [2] [\_\_] years’ experience in work of this Section.

WARRANTY

Manufacturer’s 2 year warranty for telephone entry/access and perimeter control system.

PRODUCTS

MANUFACTURERS

Contract Documents are based on products by LiftMaster. [www.liftmaster.com](http://www.liftmaster.com/)

Substitutions: [Refer to Division 01.] [Not permitted.]

TELEPHONE ENTRY CONTROL SYSTEM

Commercial and Gated Community Cloud Based Access Control/Telephone Entry System:

Model: CAPXLV Smart Video Intercom.

Local user capacity: 50,000.

Touch screen operation with USB integrated video camera.

Four primary relays and four auxiliary relays.

Compatible with MyQ Community.

Transmitters: [1-button] [3-button] credentialled; [visor.] [keychain.] [keychain with RFID.]

Internet connection: [High-speed CAT 5/6 IEEE 802.] [Wi-Fi IEEE 802]

Mounting: [42] [64] inch high pedestal.

* + - 1. Accessories:
         1. Mounting: [42], [64] inch high pedestal.
         2. CAP2D smart access two door controller.
         3. Back box and trim kit for flush mounting.
         4. Trim ring for back box and trim kit.
         5. Mini mullion reader.
         6. External keypad.
         7. Radio antenna extension kit.
         8. Wi-Fi antenna extension kit.
         9. Quick call input loop kit.
         10. Passport remote controls: Passport [Lite 1-button visor transmitter.] [Lite 1-button keychain transmitter.] [Lite 1-button keychain with prox coil.] [MAX 3 button visor transmitter.] [MAX 3 button keychain transmitter.] [MAX 3 button keychain with prox coil.]
         11. User application: myQ Community.

EXECUTION

INSTALLATION

Install in accordance with manufacturer’s instructions and approved Shop Drawings.

CLOSEOUT ACTIVITIES

Demonstration: Demonstrate system operation to Owner.

MAINTENANCE

Maintenance Service: Furnish service and maintenance of access control systems for period of 3 months after date of Substantial Completion.

END OF SECTION