LiftMaster Distributed by ZeroDocs.com

**SECTION 08 71 23 – COMMERICAL DOOR OPERATORS**

 GENERAL

 SUBMITTALS

 Action Submittals:

 Product Data: Manufacturer’s descriptive data and product attributes.

 Closeout Submittals:

 Operation and Maintenance Data.

 QUALITY ASSURANCE

 Installer Qualifications: Firm specializing in work of this Section, with minimum [2] [\_\_] years’ experience.

 WARRANTY

 Manufacturer’s [1] [2] year warranty against material and manufacturing defects.

 PRODUCTS

 MANUFACTURERS

 Contract Documents are based on products by LiftMaster. [www.LiftMaster.com](http://www.liftmaster.com)

 Substitutions: [Refer to Division 01.] [Not permitted.]

 MANUFACTURED UNITS

 Door Operators:

 Model: ATSW.

 Mounting: Ceiling.

 Drive type: Chain.

 Rated duty cycle: Maximum 8 cycles per hour and 25 cycles per day.

 Travel rate: 8 to 9 inches per second.

 Meet UL 325.

 Motor: 12 VDC, prewired, listed by Underwriters Laboratories, sized to door conditions.

 Enclosure: NEMA 1.

 Radio receiver: Security+ 2.0 receiver on-board; accept Security+ 2.0 rolling code technology remote controls.

 Internet connectivity: 50 channel FHSS myQ technology.

* + - 1. Control station: Single push button type in NEMA 1 enclosure.
			2. Remote controls: [Two button rolling code Security+ 2.0.] [Three button rolling code Security+ 2.0.] [Four button rolling code Security+ 2.0.]
			3. Entrapment protection: [Photo eyes.] [Light curtain.]
			4. Track: Steel, I-beam configuration, with automatic reconnect trolley.

 EXECUTION

 INSTALLATION

 Install in accordance with manufacturer’s instructions.

 CLOSEOUT ACTIVITIES

 Test and adjust operators for proper operation.

 Demonstration: Demonstrate operation and programming of operators to Owner.

END OF SECTION